**Start of the unit**

* Connect all hose connections
* Connect remote control cable and connections
* Check the “safety valve”
* Fill the compartments of the liner wash tank with clear water
* Check all oil levels (marked red)
* Switch “main on/off” on the main control panel to “on”
* Switch “linerwash on/off” on the main control panel to “on”
* Check the liner wash if it’s flushing
* Push “push to start” when turning the key
* Let the engine idle for 10 min.

**If the pump is running make sure that the generator is running between 1600 and 2100 rpm**

**Always switch boosterpump to “on” before running the pump**

* Check booster pressure min. 2 bar max 3.5 bar
* Never let the ignition switched on for longer than 1 minute if the engine is not running
* Lock doors at night
* Clear liner wash tank daily

**Ideal RPM for generator is between 1600-2100 rpm**

**Shut down of the unit,**

1. Put pomp in off position on panel local or remote
2. Select local on main panel
3. Stop engine on main panel
4. Turn off mass switch

**During operation frequently check:**

* Liner wash liquid level visually
* Pump general inspection
* High pressure hose ad connections
* Suction hose and connections